SUPPLIERS LETTERHEAD (With Physical Address)

Supplier / Manufacturer Name: Importer Name:

This is to certify that the materials used to manufacture the goods in this consignment contain nil asbestos and asbestos containing substances in all or any of the below forms-

|  |
| --- |
| Serpentine Group – comprised of only chrysotile (white asbestos)  Amphibole Group – comprised of amosite (brown asbestos or grey asbestos), anthophyllite, crocidolite (blue asbestos), tremolite, and actinolite.   Description of goods:     Detailed list of components and their composition: |

This declaration is valid for all orders between \_ \_ / \_ \_ / \_ \_ and \_ \_ / \_ \_ / \_ \_; if the composition, or make up of the product changes to include an asbestos product we will advise ASAP.

Signed: Printed Name:

Date of issue:

**Goods that might contain asbestos**  
Asbestos is still used outside Australia in many applications. The following imported goods are considered high risk for containing asbestos and ACM:

* Asbestos bitumen products used to damp proof
* Asbestos rope
* Asbestos tape
* Brake linings or blocks
* Cement flat sheeting or panels
* Cement pipes, tubes or fittings
* Cement shingles or tiles (external or ceiling)
* Clutch linings or brake disc pads
* Crayons
* Diaphragms
* Ducts
* Electrical cloth and tapes
* Electrical panel partitioning
* Fire blankets
* Fire curtains
* Fire-resistant building materials
* Furnaces
* Gaskets or seals
* Gloves
* Heat resistant sealing or caulking compounds
* Heating equipment
* Lagging and jointing materials
* Mastics, sealants, putties or adhesives
* Mineral samples for display or therapeutic purposes
* Mixtures containing phenol formaldehyde resin or cresylic formaldehyde resin
* Motor vehicle parts such as friction materials
* Pipe spools
* Raw materials from mining activities
* Sheet vinyl backing
* Sheeting
* Textured paints or coatings
* Tiles
* Yarn and thread, cords and string, whether or not plaited